{"text_format":"1","workbook":"xlsx","n_sheets":5,"sheets":["Revisions","Examples","Supplier Declaration","Exemptions","Part Family"],"not_rendered":{"charts":0,"images":9,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Revisions","index":0,"n_rows":19,"n_cols":3,"rows_kept":19,"cut":false,"hidden":false,"merged":[]}
["Date","Revision","Description of changes"]
["2014-08-25","A1","Adding to Revision Control (Revisions Sheet)"]
[null,null,"Added check to see if supplier accepted legal statement"]
[null,null,"Added email declaration using outlook button"]
[null,null,"Corrected Request Date and Respond by Date formatting issues"]
[null,null,"Added Auto Response Date with correct date format."]
[null,null,"Fixed wrong supplierID which caused failures in WPA queue"]
[null,null,"Added  Date format NOTE:"]
[null,null,"Added Examples Sheet"]
[null,null,"Renamed Sheet1 to Supplier Declaration"]
[null,null,"Added exemptions sheet and drop down list  in the Supplier Declaration sheet"]
[null,null,"Changed format for cells C8 and L8 to Text so the leading 0 wont be stripped."]
["2014-12-02","B1","Fixed percent sign / decimal issue"]
[null,null,"Fixed timestamp issue when loading existing XML"]
[null,null,"Added Part Family functionality"]
[null,null,"New form layout"]
[null,null,"Added massPercent as a drop down value for Materials"]
[null,null,"Added check to see if trhere was at least one material declared."]
[null,null,"Enter all product info on the Part Family sheet and not the Supplier Declaration sheet anymore."]

{"sheet":"Examples","index":1,"n_rows":59,"n_cols":1,"rows_kept":59,"cut":false,"hidden":false,"merged":[]}
["Below is an example of a part that has sub parts and materials assigned to the sub part. Note that the  Mass amount of the material eqauls 100% of the sub part."]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["In the Part Family sheet you can add more that one part which has the same material make-up. IF the mass amount is different OR the Mass Unit is different the spreadsheet will remove the sub parts. Also you will then need to use MassPercent as a UoM in the Material Section."]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["In this example you can use another UoM besides massPecent because the part family mass amount and mass units are the same"]
[]
["Part Family Sheet:"]
[]
[]
[]
[]
[]
[]
[]
["Supplier Declaration Sheet:"]

{"sheet":"Supplier Declaration","index":2,"n_rows":19,"n_cols":22,"rows_kept":19,"cut":false,"hidden":false,"merged":[[5,19,5,49],[6,2,6,4],[7,2,7,4],[8,2,8,4],[9,2,9,4],[6,10,6,13],[7,10,7,13],[8,10,8,13],[9,10,9,13],[9,8,9,9],[12,17,12,18],[6,17,11,18],[5,17,5,18],[5,1,5,4],[10,2,10,4],[11,2,11,4],[12,2,12,4],[0,1,3,7],[16,8,16,11],[16,12,16,15],[16,16,16,21],[16,1,16,3],[16,4,16,7],[2,9,2,16],[10,8,10,9],[11,8,11,9],[10,10,10,13],[11,10,11,13],[6,19,11,49],[5,8,5,13],[6,8,6,9],[7,8,7,9],[8,8,8,9]]}
[]
[]
[null,null,null,null,null,null,null,null,null,"IPC-1752A Material Declaration Generator"]
[]
[]
[null,"Requestor:",null,null,null,null,null,null,"Supplier Information:",null,null,null,null,null,null,null,null,"Legal Statement:"]
[null,"Company Name",null,null,null,null,null,null,"Company Name",null,null,null,null,null,null,null,null,"Legal Declaration"]
[null,"Company ID",null,null,null,null,null,null,"Company ID"]
[null,"Request Date",null,null,null,null,null,null,"Contact Name"]
[null,"Respond by Date",null,null,null,null,null,null,"Contact Phone"]
[null,"Contact Name",null,null,null,null,null,null,"Contact Email"]
[null,"Contact Phone",null,null,null,null,null,null,"Response Date"]
[null,"Contact Email",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Supplier Acceptance"]
[]
[null,"NOTE: The correct Date format is YYYY-MM-DD-HH:SS It is important that month, day, hour and second have two digits. In case the ones mentioned have only one digit please put zero before it. "]
[]
[null,"Product Section",null,null,"Supplier Part Section",null,null,null,"Supplier Subpart Section",null,null,null,"Material Section",null,null,null,"Substance Section"]
[null,"Part Item","Part Description","Product Units","Supplier Part","Supplier Part Description","Mass Amount ","Mass Units","Subpart Name","QTY","Mass Amount ","Mass Units","Homogeneous Material name","Material Group","Mass Amount ","Mass Units","Substance Name","CAS Number","% of Material","Ex 1","Ex 2","Ex 3 "]
[null,{"$f":" 'Part Family'!A3","v":0},{"$f":" 'Part Family'!B3","v":0},{"$f":" 'Part Family'!C3","v":0},{"$f":" 'Part Family'!D3","v":0},{"$f":" 'Part Family'!E3","v":0},{"$f":" 'Part Family'!F3","v":0},{"$f":" 'Part Family'!G3","v":0}]

{"sheet":"Exemptions","index":3,"n_rows":162,"n_cols":2,"rows_kept":162,"cut":false,"hidden":true,"merged":[]}
[1,"Mercury in compact fluorescent lamps not exceeding 5 mg per lamp / Lead, cadmium and mercury in detectors for ionising radiation"]
["1(a)","Mercury in compact fluorescent lamps < 30 W not exceeding 5 mg per lamp (in 2012: 3.5 mg, > 2012: 2.5 mg)"]
["1(b)","Mercury in compact fluorescent lamps < 50 W and > 30 W not exceeding 5 mg per lamp (> 2011: 3.5 mg)"]
["1(c)","Mercury in compact fluorescent lamps < 150 W and > 50 W not exceeding 5 mg per lamp"]
["1(d)","Mercury in compact fluorescent lamps > 150 W not exceeding 15 mg per lamp"]
["1(e)","Mercury in compact fluorescent lamps with circular or square structural shape and tube diameter < 17 mm (not exceeding 7 mg per lamp > 2011)"]
["1(f)","Mercury in compact fluorescent lamps for special purposes not exceeding 5 mg per lamp"]
["1(g)","Mercury in single capped (compact) fluorescent lamps not exceeding (per burner):For general lighting purposes less than 30 W with a lifetime equal or above 20,000 h: 3.5 mg"]
[10,"Lead and cadmium in atomic absorption spectroscopy lamps."]
[11,"Lead used in compliant pin connector systems  / Lead in alloys as a superconductor and thermal conductor in MRI"]
["11(a)","Lead used in C-press compliant pin connector systems"]
["11(b)","Lead used in other than C-press compliant pin connector systems"]
[12,"Lead as a coating material for a thermal conduction module c-ring / Lead and cadmium in metallic bonds creating superconducting magnetic circuits in MRI, SQUID, NMR (Nuclear Magnetic Resonance) or FTMS (Fourier Transform Mass Spectrometer) detectors."]
[13,"Lead in counterweights"]
["13(a)","Lead in white glasses used for optical applications"]
["13(b)","Cadmium (and lead) in filter glasses and glasses used for reflectance standards"]
[14,"Lead in solders consisting of more than two elements for the connection between the pins and the package of microprocessors with a lead content of more than 80% and less than 85% by weight / Lead in single crystal piezoelectric materials for ultrasonic transducers"]
[15,"Lead in solders to complete a viable electrical connection between semiconductor die and carrier within integrated circuit Flip Chip packages / Lead in solders for bonding to ultrasonic transducers"]
[16,"Lead used in linear incandescent lamps with silicate coated tubes / Mercury in very high accuracy capacitance and loss measurement bridges and in high frequency RF switches and relays in monitoring and control instruments not exceeding 20 mg of mercury per switch or relay"]
[17,"Lead halide as radiant agent in High Intensity Discharge (HID) lamps used for professional reprography applications / Lead in solders in portable emergency defibrillators"]
[18,"Lead as activator in the fluorescent powder (1 % lead by weight or less) of discharge lamps when used as sun tanning lamps containing phosphors such as BSP (BaSi2O5:Pb) as well as when used as speciality lamps for diazo-printing reprography, lithography, insect traps, photochemical and curing processes containing phosphors such as SMS ((Sr,Ba)2MgSi2O7:Pb)"]
["18(a)","Lead as activator in the fluorescent powder (1 % lead by weight or less) of discharge lamps when used as speciality lamps for diazoprinting reprography, lithography, insect traps, photochemical and curing processes containing phosphors such as SMS ((Sr,Ba)2MgSi2O7:Pb)"]
["18(b)","Lead as activator in the fluorescent powder (1% lead by weight or less) of discharge lamps when used as sun tanning lamps containing phosphors such as BSP (BaSi2O5:Pb)"]
[19,"Lead with PbBiSn-Hg and PbInSn-Hg in specific compositions as main amalgam and with PbSn-Hg as auxiliary amalgam in very compact Energy Saving Lamps (ESL) / Lead in Liquid crystal on silicon (LCoS) displays"]
["1a","Lead and cadmium in ion selective electrodes including glass of pH electrodes"]
["1b","Lead anodes in electrochemical oxygen sensors"]
["1c","Lead, cadmium and mercury in infra-red light detectors"]
["1d","Mercury in reference electrodes: low chloride mercury chloride, mercury sulphate and mercury oxide"]
[2,"Lead bearings in X-ray tubes"]
["2(a)(1)","Mercury in straight fluorescent lamps with tri-band phosphor for general purposes with normal lifetime and a tube diameter < 9 mm (e.g. T2) not exceeding 5 mg per lamp (> 2011: 4 mg)"]
["2(a)(2)","Mercury in straight fluorescent lamps with tri-band phosphor for general purposes with normal lifetime and a tube diameter < 17 mm and > 9 mm (e.g. T5) not exceeding 5 mg per lamp (> 2011: 3 mg)"]
["2(a)(3)","Mercury in straight fluorescent lamps with tri-band phosphor for general purposes with normal lifetime and a tube diameter < 28 mm and > 17 mm (e.g. T8) not exceeding 5 mg per lamp (> 2011: 3.5 mg)"]
["2(a)(4)","Mercury in straight fluorescent lamps with tri-band phosphor for general purposes with normal lifetime and a tube diameter > 28 mm (e.g. T12) not exceeding 5 mg per lamp (> 2012: 3.5 mg)"]
["2(a)(5)","Mercury in straight fluorescent lamps with tri-band phosphor for general purposes with long lifetime (> 25000h) not exceeding 8 mg per lamp (> 2011: 5 mg)"]
["2(b)(1)","Linear halophosphate lamps with tube diameter > 28 mm (e.g. T10 and T12) not exceeding 10 mg in halophosphate lamps"]
["2(b)(2)","Mercury in non-linear halophosphate lamps (all diameters) not exceeding 15 mg in halophosphate lamps"]
["2(b)(3)","Mercury in non-linear tri-band phosphor lamps with tube diameter > 17 mm (e.g. T9) (> 2011: not exceeding 15 mg per lamp)"]
["2(b)(4)","Mercury in lamps for other general lighting and special purposes (e.g. induction lamps) (> 2011: not exceeding 15 mg per lamp)"]
[20,"Lead oxide in glass used for bonding front and rear substrates of flat fluorescent lamps used for Liquid Crystal Displays (LCD) / Cadmium in X-ray measurement filters"]
[21,"Lead and cadmium in printing inks for the application of enamels on borosilicate glass / Cadmium in phosphor coatings in image intensifiers for X-ray images until 31 December 2019 and in spare parts for X-ray systems placed on the EU market before 1 January 2020."]
[22,"Lead as impurity in RIG (rare earth iron garnet) Faraday rotators used for fibre optic communications systems / Lead acetate marker for use in stereotactic head frames for use with CT and MRI and in positioning systems for gamma beam and particle therapy equipment. Expires on 30 June 2021."]
[23,"Lead in finishes of fine pitch components other than connectors with a pitch of 0.65 mm or less with NiFe lead frames and lead in finishes of fine pitch components other than connectors with a pitch of 0.65 mm or less with copper lead frames / Lead as an alloying element for bearings and wear surfaces in medical equipment exposed to ionising radiation. Expires on 30 June 2021."]
[24,"Lead in solders for the soldering to machined through hole discoidal and planar array ceramic multilayer capacitors / Lead enabling vacuum tight connections between aluminium and steel in X-ray image intensifiers. Expires on 31 December 2019."]
[25,"Lead oxide in plasma display panels (PDP) and surface conduction electron emitter displays (SED) used in structural elements; notably in the front and rear glass dielectric layer, the bus electrode, the black stripe, the address electrode, the barrier ribs, the seal frit and frit ring as well as in print pastes / Lead in the surface coatings of pin connector systems requiring nonmagnetic connectors which are used durably at a temperature below -20&#176;C under normal operating and storage conditions. Expires on 30 June 2021."]
[26,"Lead in solders on printed circuit boards, termination coatings of electrical and electronic components and coatings of printed circuit boards, solders for connecting wires and cables, solders connecting transducers and sensors, that are used durably at a temperature below -20&#176;C under normal operating and storage conditions. Expires on 30 June 2021. / Lead oxide in the glass envelope of Black Light Blue (BLB) lamps"]
[27,"Lead in solders, termination coatings of electrical and electronic components and PCBs, wire connections, shields and enclosed connectors used in (a) magnetic fields within sphere of 1 m around isocentre of magnet in medical MRI equipment, including patient monitors for use within sphere, or (b) magnetic fields within 1 m of the external surfaces of cyclotron magnets, magnets for beam transport beam direction control applied for particle therapy. Expires on 30 June 2020. / Lead alloys as solder for transducers used in high-powered (designated to operate for several hours at acoustic power levels of 125 dB SPL and above) loudspeakers"]
[28,"Lead in solders for mounting cadmium telluride and cadmium zinc telluride digital array detectors to printed circuit boards. Expires on 31 December 2017. / Hexavalent chromium in corrosion preventive coatings of unpainted metal sheetings and fasteners used for corrosion protection and Electromagnetic Interference Shielding in equipment falling under category three of Directive 2002/96/EC (IT and telecommunications equipment). Exemption granted until 1 July 2007"]
[29,"Lead in alloys, as a superconductor or thermal conductor, used in cryo-cooler cold heads and/or in cryo-cooled cold probes and/or in cryo-cooled equipotential bonding systems, in medical devices (category 8) and/or in industrial monitoring and control instruments. Expires on 30 June 2021. / Lead bound in crystal glass as defined in Annex I (Categories 1, 2, 3 and 4) of Council Directive 69/493/EEC (*)"]
["2a","Mercury in straight fluorescent lamps for general purposes not exceeding 10 mg. in halophosphate lamps"]
["2b","Mercury in straight fluorescent lamps for general purposes not exceeding 5 mg. in triphosphate lamps with a normal lifetime"]
["2c","Mercury in straight fluorescent lamps for general purposes not exceeding 8 mg. in triphosphate lamps with long lifetime"]
[3,"Lead in electromagnetic radiation amplification devices: micro-channel plate and capillary plate. / Mercury in straight fluorescent lamps for special purposes"]
["3(a)","Mercury in short length (< 500 mm) cold cathode fluorescent lamps and external electrode fluorescent lamps (CCFL and EEFL) for special purposes  (> 2011: not exceeding 3.5 mg per lamp)"]
["3(b)","Mercury in medium length (greater than 500 mm and < 1,500 mm) cold cathode fluorescent lamps and external electrode fluorescent lamps (CCFL and EEFL) for special purposes (> 2011: not exceeding 5 mg per lamp)"]
["3(c)","Mercury in long length (> 1,500 mm) cold cathode fluorescent lamps and external electrode fluorescent lamps (CCFL and EEFL) for special purposes (> 2011: not exceeding 13 mg per lamp)"]
[30,"Cadmium alloys as electrical/mechanical solder joints to electrical conductors located directly on the voice coil in transducers used in high-powered loudspeakers with sound pressure levels of 100 dB and more / Hexavalent chromium in alkali dispensers used to create photocathodes in X-ray image intensifiers until 31 December 2019 and in spare parts for X-ray systems placed on the EU market before 1 January 2020."]
[31,"Lead, cadmium and hexavalent chromium in reused spare parts, recovered from medical devices placed on the market before 22 July 2014 and used in category 8 equipment placed on the market before 22 July 2021, provided that reuse takes place in auditable closed-loop business-to-business return systems, and that the reuse of parts is notified to the consumer. Expires on 21 July 2021. / Lead in soldering malterials in merucry free flat fluorescent lamps"]
[32,"Lead in solders on printed circuit boards of detectors and data acquisition units for Positron Emission Tomographs which are integrated into Magnetic Resonance Imaging equipment. Expires on 31 December 2019. / Lead Oxide in seal frit used for making window assemblies for Argon and Krypton laser tubes."]
[33,"Lead in solders on populated printed circuit boards used in Directive 93/42/EEC class IIa and IIb mobile medical devices other than portable emergency defibrillators. Expires on 30 June 2016 for class IIa and on 31 December 2020 for class IIb. / Lead in solders for the soldering of thin copper wires of 100 um diameter and less in power transformers"]
[34,"Lead as an activator in the fluorescent powder of discharge lamps when used for extracorporeal photopheresis lamps containing BSP (BaSi 2 O 5 :Pb) phosphors. Expires on 22 July 2021. Lead in cermet based trimmer potentiometer elements"]
[35,"Cadmium in photoresistors for optocouplers applied in professional audio equipment until 31 December 2009 / Mercury in cold cathode fluorescent lamps for back-lighting liquid crystal displays, not exceeding 5 mg per lamp, used in industrial monitoring and control instruments placed on the market before 22 July 2017 Expires on 21 July 2024"]
[36,"Lead used in other than C-press compliant pin connector systems for industrial monitoring and control instruments. / Mercury used as a cathode sputtering inhibitor in DC plasma displays with a content up to 30 mg per display"]
[37,"Lead in platinum electrodes used for conductivity measurements where one of the following apply: a) wide-range measurements with a conductivity range between 0.1 mS/m and 5mS/m, b)measurement of solution with pH <1 or >13 or for halogen gas, c) measurements of conduct above 100 mS/m for portable instruments / Lead in the plating layer of high voltage diodes on the basis of a zinc borate glass body"]
[38,"Lead in solder in one interface of large area stacked die elements with more than 500 interconnects per interface which are used in X-ray detectors of computed tomography and X-ray systems. Expires on 31 December 2019.  May be used after that date in spare parts for CT and X-ray systems placed on the market before 1 January 2020. / Cadmium and Cadmium oxide in thick film pasts used on aluminum bonded beryllium oxide"]
[39,"Lead in micro-channel plates (MCPs) in equipment where one of the following is present: a) a compact size detector of the detector for electrons or ions, with space limited to a maximum of 6mm  b) two-dimensional  spatial resolution for detecting electrons or ions where a response time is less than 25ns or sample detection area is >149 mm2 c)response time is shorter than 5ns d) sample detection is >314 mm2 e) multi factor >4x10^7 / Cadmium in colour-converting II-VI LEDs (less than 10 micrograms Cd per mm 2 of light-emitting area) for use in solid state illumination or display system until 1 July 2014"]
[4,"Lead in glass frit of X-ray tubes and image intensifiers and lead in glass frit binder for assembly of gas lasers and for vacuum tubes that convert electromagnetic radiation into electrons.. / Mercury in other lamps not specifically mentioned in this list"]
["4(a)","Mercury in other low pressure discharge lamps (> 2011: not exceeding 15 mg per lamp)"]
["4(b)-I","Mercury in high Pressure Sodium (vapour) lamps for general lighting purposes < 155 W with improved colour rendering index Ra > 60 (> 2011: not exceeding 30 mg per lamp)"]
["4(b)-II","Mercury in high Pressure Sodium (vapour) lamps for general lighting purposes < 405 W and > 155 W with improved colour rendering index Ra > 60 (> 2011: not exceeding 40 mg per lamp)"]
["4(b)-III","Mercury in high Pressure Sodium (vapour) lamps for general lighting purposes > 405 W with improved colour rendering index Ra > 60 (> 2011: not exceeding 40 mg per lamp)"]
["4(c)-I","Mercury in other High Pressure Sodium (vapour) lamps for general lighting purposes < 155W (> 2011: not exceeding 25 mg per lamp)"]
["4(c)-II","Mercury in other High Pressure Sodium (vapour) lamps for general lighting purposes < 155W (> 2011: not exceeding 30 mg per lamp)"]
["4(c)-III","Mercury in other High Pressure Sodium (vapour) lamps for general lighting purposes < 155W (> 2011: not exceeding 40 mg per lamp)"]
["4(d)","Mercury in High Pressure Mercury (vapour) lamps (HPMV)"]
["4(e)","Mercury in metal halide lamps (MH)"]
["4(f)","Mercury in other discharge lamps not specifically mentioned in this list"]
["4(g)","Mercury in hand crafted luminous discharge tubes used for signs, decorative or architectural and specialist lighting and light-artwork, where the mercury content shall be limited as follows: (a) 20 mg per electrode pair + 0,3 mg per tube length in cm, but not more than 80 mg, for outdoor applications and indoor applications exposed to temperatures below 20 &#176;C; (b) 15 mg per electrode pair + 0,24 mg per tube length in cm, but not more than 80 mg, for all other indoor applications"]
[40,"Lead in dielectric ceramic in capacitors for a rated voltage of less than 125 V AC or 250 V DC for industrial monitoring and control instruments. Expires on 31 December 2020.  May be used after that date in spare parts for industrial monitoring and control instruments placed on the market before 1 January 2021. / Cadmium in photoresistors for analogue optocouplers applied in professional audio equipment"]
[41,"Lead in solders and termination finishes of electrical and electronic components and finishes of printed circuit boards used in ignition modules and other electrical and electronic engine control systems, which for technical reasons must be mounted directly on or in the crankcase or cylinder of hand-held combustion engines (classes SH:1, SH:2, SH:3 of Directive 97/68/EC of the European Parliament and of the Council(*)"]
[5,"Lead in glass of cathode ray tubes, electronic components and fluorescent tubes. / Lead in shielding for ionising radiation."]
["5(a)","Lead in glass of cathode ray tubes"]
["5(b)","Lead in glass of fluorescent tubes not exceeding 0.2% by weight"]
[6,"Lead in X-ray test objects"]
["6(a)","Lead as an alloying element in steel containing up to 0.35% lead by weight"]
["6(b)","Lead as an alloying element in aluminum containing up to 0.4% lead by weight"]
["6(c)","Lead as an alloying element in copper containing up to 4% lead by weight"]
[7,"Lead stearate X-ray diffraction crystals"]
["7(a)","Lead in high melting temperature type solders (i.e. lead based solder alloys containing 85% by weight or more lead)"]
["7(b)","Lead in solders for servers, storage and storage array systems, network infrastructure equipment for switching, signalling, transmission as well as network management for telecommunications"]
["7(c)-I","Electrical and electronic components containing lead in a glass or ceramic other than dielectric ceramic in capacitors, e.g. piezoelectronic devices, or in a glass or ceramic matrix compound"]
["7(c)-II","Lead in dielectric ceramic in capacitors for a rated voltage of 125 V AC or 250 V DC or higher"]
["7(c)-III","Lead in dielectric ceramic in capacitors for a rated voltage of less than 125 V AC or 250 V DC"]
["7(c)-IV","Lead in PZT based dielectric ceramic materials for capacitors being part of integrated circuits or discrete semiconductors"]
["7c","Lead in electronic ceramic parts (e.g. piezoelectronic devices)"]
[8,"Cadmium and its compounds in electrical contacts and cadmium plating except for applications banned under Directive 91/338/EEC amending Directive 76/769/EEC relating to restrictions on the marketing and use of certain dangerous substances and preparations piezoelectronic devices) / Radioactive cadmium isotope source for portable X-ray fluorescence spectrometers"]
["8(a)","Cadmium and its compounds in one shot pellet type thermal cut-offs"]
["8(b)","Cadmium and its compounds in electrical contacts"]
[9,"Hexavalent chromium as an anti-corrosion of the carbon steel cooling system in absorption refrigerators / Cadmium in helium-cadmium lasers"]
["9(b)","Lead in lead/bronze bearing shells and bushes"]
["9a","Deca BDE in polymeric applications"]
["RA1","Uses in the immediate packaging of medicinal products covered under Regulation (EC) No 726/2004, Directive 2001/82/EC, and/or Directive 2001/83/EC"]
["RR10a","Not used in jokes and hoaxes"]
["RR10b","Used in stink bombs containing not more than 1.5 ml of liquid"]
["RR11a","Not used in jokes and hoaxes"]
["RR11b","Used in stink bombs containing not more than 1.5 ml of liquid"]
["RR16","Not intended for use as paint"]
["RR17","Not intended for use as paint"]
["RR18","Used according to Reach Restricted Directive (Regulation No 552/2009)"]
["RR19","Used according to Reach Restricted Directive (Regulation No 552/2009)"]
["RR2","Not used as propellant in aerosols"]
["RR20a","Used according to Reach Restricted Directive (Regulation No 276/2010)"]
["RR20b","Used according to Reach Restricted Directive (Regulation No 276/2010)"]
["RR20c","Used according to Reach Restricted Directive (Regulation No 276/2010)"]
["RR21","Intended solely for conversion into articles, among which this substance will no longer feature in a concentration equal to or greater than 0.1%"]
["RR23","Used according to Reach Restricted Directive (Regulation No 552/2009)"]
["RR23a","Articles and components used in the aeronautical, aerospace, mining, offshore and nuclear sectors or where electrical contacts require high reliability"]
["RR24a","Plant and machinery already in service on 18 June 1994, until such plant and machinery is disposed of"]
["RR24b","Maintenance of plant and machinery already in service within a Member State on 18 June 1994"]
["RR27","Not used in direct contact with skin or having a release rate <0.5 micro g/wk>"]
["RR28","Used according to Reach Restricted Directive (Regulation No 552/2009)"]
["RR3","Used according to Reach Restricted Directive (Regulation No 552/2009)"]
["RR31","Used according to Reach Restricted Directive (Regulation No 552/2009)"]
["RR32","Used according to Reach Restricted Directive (Regulation No 552/2009)"]
["RR34","Used according to Reach Restricted Directive (Regulation No 552/2009)"]
["RR35","Used according to Reach Restricted Directive (Regulation No 552/2009)"]
["RR36","Used according to Reach Restricted Directive (Regulation No 552/2009)"]
["RR37","Used according to Reach Restricted Directive (Regulation No 552/2009)"]
["RR38","Used according to Reach Restricted Directive (Regulation No 552/2009)"]
["RR4","Not used in textile articles with skin contact"]
["RR40","Used according to Reach Restricted Directive (Regulation No 552/2009)"]
["RR41","Is not intended for the manufacturing or processing of non-ferrous metals"]
["RR43","Not used in textile and leather articles"]
["RR45","Used according to Reach Restricted Directive (Regulation No 552/2009)"]
["RR46","Used according to Reach Restricted Directive (Regulation No 552/2009)"]
["RR47a","Not used in cement"]
["RR47b","Used in controlled closed and totally automated processes"]
["RR48","Not used in adhesives or spray paints intended for supply to the general public"]
["RR49","Process solvent in closed chemical applications for chlorination reactions or the manufacture of 1,3,5-triamino-2,4,6-trinitrobenzene (TATB)"]
["RR50","Not used in or for the production of tires"]
["RR51","Not used in toys and childcare articles"]
["RR52","Used according to Reach Restricted Directive (Regulation No 276/2010)"]
["RR54","Not used as a constituent of paints, paint strippers, cleaning agents, self-shining emulsions or floor sealants"]
["RR55","Used according to Reach Restricted Directive (Regulation No 552/2009)"]
["RR56","Used according to Reach Restricted Directive (Regulation No 552/2009)"]
["RR57","Used according to Reach Restricted Directive (Regulation No 552/2009)"]
["RR58","Used for agriculture as described in Reach Restricted Directive (Regulation No 552/2009)"]
["RR59","Used according to Reach Restricted Directive (Regulation No 276/2010)"]
["RR5a","Not used in toys and concentration not above 1000 ppm"]
["RR5b","Motor fuels which are covered by Directive 98/70/EC"]
["RR60","Not used as a substance or constituent of mixtures in a concentration equal to or greater than 0,1 % by weight for grouting applications"]
["RR62a","Articles or any parts thereof containing one or more of these substances shall not be placed on the market after 10 October 2017 if the concentration of mercury in the articles or any part thereof is equal to or greater than 0,01 % by weight."]
["RR62b","Articles or any parts thereof containing one or more of these substances shall not be placed on the market after 10 October 2017 if the concentration of mercury in the articles or any part thereof is equal to or greater than 0,01 % by weight."]
["RR63a","Not used in jewelry or jewelry making"]
["RR63b","Used for crystal glass as defined in Annex I (categories 1, 2, 3 and 4) to Council Directive 69/493/EEC (*);"]
["RR63c","Used for internal components of watch timepieces inaccessible to consumers"]
["RR63d","Use for non-synthetic or reconstructed precious and semiprecious stones (CN code 7103, as established by Regulation (EEC) No 2658/87), unless they have been treated with lead or its compounds or mixtures containing these substances"]
["RR63e","Used for enamels, defined as vitrifiable mixtures resulting from the fusion, vitrification or sintering of minerals melted at a temperature of at least 500 Â°C"]
["RR63f","Used in jewelry placed on the market for the first time before 9 October 2013 and jewelry articles produced before 10 December 1961."]
["RR7","Not used in textile articles with skin contact"]
["RR8","Not used in textile articles with skin contact"]
["RR9a","Not used in jokes and hoaxes"]
["RR9b","Used in stink bombs containing not more than 1.5 ml of liquid"]

{"sheet":"Part Family","index":4,"n_rows":2,"n_cols":7,"rows_kept":2,"cut":false,"hidden":false,"merged":[[0,0,0,2],[0,3,0,6]]}
["Product Family Section",null,null,"Supplier Part Section"]
["Part Item #","Part Description","Product Units","Supplier Part","Supplier Part Description","Mass Amount ","Mass Units"]