getPinConfig[GPIO\_09]: "O,D,0"

getTWPinConfigs(GPIO\_09): O,D,0

getPinNode: {

"altPinName": "RPI\_GPIO\_P1\_XX",

"pinConf": "O,D,0",

"pinDirection": ["I", "O"],

"pinType": ["D"]

}

getPinConfig[GPIO\_11]: "O,D,0"

getTWPinConfigs(GPIO\_11): O,D,0

getPinNode: {

"altPinName": "RPI\_GPIO\_P1\_XX",

"pinConf": "O,D,0",

"pinDirection": ["I", "O"],

"pinType": ["D"]

}

getPinConfig[GPIO\_18]: "O,D,0"

getTWPinConfigs(GPIO\_18): O,D,0

getPinNode: {

"altPinName": "RPI\_GPIO\_P1\_XX",

"pinConf": "O,D,0",

"pinDirection": ["I", "O"],

"pinType": ["D"]

}

getPinConfig[GPIO\_23]: "O,D,0"

getTWPinConfigs(GPIO\_23): O,D,0

getPinNode: {

"altPinName": "RPI\_GPIO\_P1\_XX",

"pinConf": "O,D,0",

"pinDirection": ["I", "O"],

"pinType": ["D"]

}

getPinConfig[GPIO\_24]: "O,D,0"

getTWPinConfigs(GPIO\_24): O,D,0

getPinNode: {

"altPinName": "RPI\_GPIO\_P1\_XX",

"pinConf": "O,D,0",

"pinDirection": ["I", "O"],

"pinType": ["D"]

}

getPinConfig[GPIO\_25]: "O,D,0"

getTWPinConfigs(GPIO\_25): O,D,0

getPinNode: {

"altPinName": "RPI\_GPIO\_P1\_XX",

"pinConf": "O,D,0",

"pinDirection": ["I", "O"],

"pinType": ["D"]

}

getPinConfig[GPIO\_08]: "O,D,0"

getTWPinConfigs(GPIO\_08): O,D,0

getPinNode: {

"altPinName": "RPI\_GPIO\_P1\_XX",

"pinConf": "O,D,0",

"pinDirection": ["I", "O"],

"pinType": ["D"]

}

getPinConfig[GPIO\_07]: "O,D,0"

getTWPinConfigs(GPIO\_07): O,D,0

[WARN ] 2016-04-11 09:57:01,581: api:sendMessageBlocking: Received Response to Message 134. Code: 160

creating property list....(nil)Added Hostname...0x40624

Added IP Address...0x4062c

Staring Board Specific properties...0x763005b0

localTargetPin=0

localTargetPin=1

localTargetPin=4

localTargetPin=17

localTargetPin=21

localTargetPin=22

localTargetPin=10

localTargetPin=9

localTargetPin=11

localTargetPin=18

localTargetPin=23

localTargetPin=24

localTargetPin=25

localTargetPin=8

localTargetPin=7

getPinNode: {

"altPinName": "RPI\_GPIO\_P1\_XX",

"pinConf": "O,D,0",

"pinDirection": ["I", "O"],

"pinType": ["D"]

}

getPinConfig[GPIO\_00]: "O,D,0"

getTWPinConfigs(GPIO\_00): O,D,0

getPinNode: {

"altPinName": "RPI\_GPIO\_P1\_XX",

"pinConf": "O,D,0",

"pinDirection": ["I", "O"],

"pinType": ["D"]

}

getPinConfig[GPIO\_01]: "O,D,0"

getTWPinConfigs(GPIO\_01): O,D,0

getPinNode: {

"altPinName": "RPI\_GPIO\_P1\_XX",

"pinConf": "O,D,0",

"pinDirection": ["I", "O"],

"pinType": ["D"]

}

getPinConfig[GPIO\_04]: "O,D,0"

getTWPinConfigs(GPIO\_04): O,D,0

getPinNode: {

"altPinName": "RPI\_GPIO\_P1\_XX",

"pinConf": "O,D,0",

"pinDirection": ["I", "O"],

"pinType": ["D"]

}

getPinConfig[GPIO\_17]: "O,D,0"

getTWPinConfigs(GPIO\_17): O,D,0

getPinNode: {

"altPinName": "RPI\_GPIO\_P1\_XX",

"pinConf": "O,D,0",

"pinDirection": ["I", "O"],

"pinType": ["D"]

}

getPinConfig[GPIO\_21]: "O,D,0"

getTWPinConfigs(GPIO\_21): O,D,0

getPinNode: {

"altPinName": "RPI\_GPIO\_P1\_XX",

"pinConf": "O,D,0",

"pinDirection": ["I", "O"],

"pinType": ["D"]

}

getPinConfig[GPIO\_22]: "O,D,0"

getTWPinConfigs(GPIO\_22): O,D,0

getPinNode: {

"altPinName": "RPI\_GPIO\_P1\_XX",

"pinConf": "O,D,0",

"pinDirection": ["I", "O"],

"pinType": ["D"]

}

getPinConfig[GPIO\_10]: "O,D,0"

getTWPinConfigs(GPIO\_10): O,D,0

getPinNode: {

"altPinName": "RPI\_GPIO\_P1\_XX",

"pinConf": "O,D,0",

"pinDirection": ["I", "O"],

"pinType": ["D"]

}

getPinConfig[GPIO\_09]: "O,D,0"

getTWPinConfigs(GPIO\_09): O,D,0

getPinNode: {

"altPinName": "RPI\_GPIO\_P1\_XX",

"pinConf": "O,D,0",

"pinDirection": ["I", "O"],

"pinType": ["D"]

}

getPinConfig[GPIO\_11]: "O,D,0"

getTWPinConfigs(GPIO\_11): O,D,0

getPinNode: {

"altPinName": "RPI\_GPIO\_P1\_XX",

"pinConf": "O,D,0",

"pinDirection": ["I", "O"],

"pinType": ["D"]

}

getPinConfig[GPIO\_18]: "O,D,0"

getTWPinConfigs(GPIO\_18): O,D,0

getPinNode: {

"altPinName": "RPI\_GPIO\_P1\_XX",

"pinConf": "O,D,0",

"pinDirection": ["I", "O"],

"pinType": ["D"]

}

getPinConfig[GPIO\_23]: "O,D,0"

getTWPinConfigs(GPIO\_23): O,D,0

getPinNode: {

"altPinName": "RPI\_GPIO\_P1\_XX",

"pinConf": "O,D,0",

"pinDirection": ["I", "O"],

"pinType": ["D"]

}

getPinConfig[GPIO\_24]: "O,D,0"

getTWPinConfigs(GPIO\_24): O,D,0

getPinNode: {

"altPinName": "RPI\_GPIO\_P1\_XX",

"pinConf": "O,D,0",

"pinDirection": ["I", "O"],

"pinType": ["D"]

}

getPinConfig[GPIO\_25]: "O,D,0"

getTWPinConfigs(GPIO\_25): O,D,0

getPinNode: {

"altPinName": "RPI\_GPIO\_P1\_XX",

"pinConf": "O,D,0",

"pinDirection": ["I", "O"],

"pinType": ["D"]

}

getPinConfig[GPIO\_08]: "O,D,0"

getTWPinConfigs(GPIO\_08): O,D,0

getPinNode: {

"altPinName": "RPI\_GPIO\_P1\_XX",

"pinConf": "O,D,0",

"pinDirection": ["I", "O"],

"pinType": ["D"]

}

getPinConfig[GPIO\_07]: "O,D,0"

getTWPinConfigs(GPIO\_07): O,D,0

[WARN ] 2016-04-11 09:58:19,928: handleMessage: Could not find matching request for Response message ID: 144